==== Address Map Table (AMT)

Defined by ARIB in <<ARIB-B10>>.

[source,xml]
----
<AMT version="uint5, default=0" current="bool, default=true">

  <!-- One per service -->
  <service service_id="uint16, required"
           src="ip-address/prefix, required"
           dst="ip-address/prefix, required">
    <private_data>
      Hexadecimal content
    </private_data>
  </service>

</AMT>
----

In each `<service>`, the `src` and `dst` addresses must have the same type, IPv4 or IPv6.
