==== MPE-IFEC Table

Defined by DVB in <<ETSI-102-772>>.

[source,xml]
----
<MPE_IFEC burst_number="uint8, required" IFEC_burst_size="uint8, required">

  <!-- One per burst (one burst per section) -->
  <burst>
    <real_time_parameters
        delta_t="uint12, required"
        MPE_boundary="bool, required"
        frame_boundary="bool, required"
        prev_burst_size="uint18, required"/>
    <IFEC_data>
      Hexadecimal content
    </IFEC_data>
  </burst>

</MPE_IFEC>
----
