==== MPE-FEC Table

Defined by DVB in <<ETSI-301-192>>.

[source,xml]
----
<MPE_FEC padding_columns="uint8, required">

  <!-- One per column (one column per section) -->
  <column>
    <real_time_parameters
        delta_t="uint12, required"
        table_boundary="bool, required"
        frame_boundary="bool, required"
        address="uint18, required"/>
    <rs_data>
      Hexadecimal content
    </rs_data>
  </column>

</MPE_FEC>
----
