==== Container Table

Defined by DVB in <<ETSI-102-323>> (TV-Anytime).

[source,xml]
----
<container_table version="uint5, default=0"
     current="bool, default=true"
     container_id="uint16, required">

  <!-- Complete compression_wrapper (see ETSI TS 102 323, 7.3.1.5) -->
  <compression_wrapper>
    Hexadecimal content
  </compression_wrapper>

</container_table>
----
