==== ISDB_cable_TS_division_system_descriptor

Defined by JCTEA in <<JCTEA-003>>.

[source,xml]
----
<ISDB_cable_TS_division_system_descriptor>

  <!-- One per carrier -->
  <carrier
      frequency="uint, frequency in Hz, required"
      frame_type="uint4, required"
      FEC_outer="uint4, required"
      modulation="uint8, required"
      symbol_rate="uint, in symbols/second, required"
      FEC_inner="uint4, default=15">

    <future_use_data>
      Hexadecimal content
    </future_use_data>

    <!-- One per service in the carrier -->
    <service id="uint16, required"/>

  </carrier>

</ISDB_cable_TS_division_system_descriptor>
----
