==== dsmcc_caching_proiority_descriptor

Defined by DVB in <<ETSI-102-809>>.

[source,xml]
----
<dsmcc_caching_priority_descriptor
    priority_value="uint8, required"
    transparency_level="uint8, required"/>
----
