==== Data Event Table (DET)

Defined by ATSC in <<ATSC-A90>>.

[source,xml]
----
<DET version="uint5, default=0"
     source_id="uint16, required"
     protocol_version="uint8, default=0">

  <!-- One per data event -->
  <data data_id="uint14, required"
        start_time="YYYY-MM-DD hh:mm:ss, required"
        ETM_location="uint2, required"
        length_in_seconds="uint20, required">

    <!-- Optional ATSC multiple_string_structure() containing one or more strings -->
    <title_text>
      <string language="char3, required" text="string, required"/>
    </title_text>

    <!-- Data event descriptors loop -->
    <DESCRIPTOR_LIST>

  </data>

</DET>
----
