==== ATSC_PID_count_descriptor

Defined by ATSC in <<ATSC-A90>>.

[source,xml]
----
<ATSC_PID_count_descriptor
    total_number_of_PIDs="uint13, default=0"
    min_number_of_PIDs="uint13, default=0"/>
----
