==== ATSC_download_descriptor

Defined by ATSC in <<ATSC-A90>>.

[source,xml]
----
<ATSC_download_descriptor
    download_id="uint32, required"
    carousel_period="uint32, default=0"
    control_msg_time_out_value="uint32, default=0"/>
----
