==== ATSC_stuffing_descriptor

Defined by ATSC in <<ATSC-A65>>.

This is the ATSC version of the `stuffing_descriptor`.
DVB uses a distinct descriptor.

[source,xml]
----
<ATSC_stuffing_descriptor>
  Hexadecimal content
</ATSC_stuffing_descriptor>
----
