==== IP/MAC Notification Table (INT)

Defined by DVB in <<ETSI-301-192>>.

[source,xml]
----
<INT version="uint5, default=0"
     current="bool, default=true"
     action_type="uint8, default=0x01"
     processing_order="uint8, default=0x00"
     platform_id="uint24, required">

  <!-- Plaform-level descriptors -->
  <DESCRIPTOR_LIST>

  <!-- One per device -->
  <device>
    <target>
      <DESCRIPTOR_LIST>
    </target>
    <operational>
      <DESCRIPTOR_LIST>
    </operational>
  </device>

</INT>
----
