==== target_IP_source_slash_descriptor

Defined by DVB in <<ETSI-301-192>>.
Must be in an INT (table id 0x4C).

[source,xml]
----
<target_IP_source_slash_descriptor>
  <!-- One per pair of IPv4 address: -->
  <address
      IPv4_source_addr="IPv4 address, required"
      IPv4_source_slash_mask="uint8, required"
      IPv4_dest_addr="IPv4 address, required"
      IPv4_dest_slash_mask="uint8, required"/>
</target_IP_source_slash_descriptor>
----
