==== CI_ancillary_data_descriptor

Defined by DVB in <<ETSI-300-468>>.

[source,xml]
----
<CI_ancillary_data_descriptor>
  <ancillary_data>
    Hexadecimal content
  </ancillary_data>
</CI_ancillary_data_descriptor>
----
