==== dsmcc_subgroup_association_descriptor

Defined by DVB in <<ETSI-102-006>>.
Must be in a DSI (table id 0x3B).

[source,xml]
----
<dsmcc_subgroup_association_descriptor subgroup_tag="uint40, required"/>
----
