==== CP_identifier_descriptor

Defined by DVB in <<ETSI-300-468>>.

[source,xml]
----
<CP_identifier_descriptor>
  <!-- One per CP system -->
  <CP_system_id value="uint16, required"/>
</CP_identifier_descriptor>
----
