==== ECM_repetition_rate_descriptor

Defined by DVB in <<ETSI-301-192>>.

[source,xml]
----
<ECM_repetition_rate_descriptor
    CA_system_id="uint16, required"
    ECM_repetition_rate="uint16, required">
  <private_data>
    Hexadecimal content
  </private_data>
</ECM_repetition_rate_descriptor>
----
