==== SSU_location_descriptor

Defined by DVB in <<ETSI-102-006>>.
Must be in a UNT (table id 0x4B).

[source,xml]
----
<SSU_location_descriptor
    data_broadcast_id="uint16, required"
    association_tag="uint16, optional">

  <private_data>
    Hexadecimal content
  </private_data>

</SSU_location_descriptor>
----
