==== content_descriptor

Defined by DVB in <<ETSI-300-468>>.

[source,xml]
----
<content_descriptor>

  <!-- One per classification -->
  <content content_nibble_level_1="uint4, required"
           content_nibble_level_2="uint4, required"
           user_byte="uint8, required"/>

</content_descriptor>
----
