==== application_recording_descriptor

Defined by DVB in <<ETSI-102-809>>.
Must be in an AIT (table id 0x74).

[source,xml]
----
<application_recording_descriptor
    scheduled_recording="bool, required"
    trick_mode_aware="bool, required"
    time_shift="bool, required"
    dynamic="bool, required"
    av_synced="bool, required"
    initiating_replay="bool, required">
  <!-- One per label -->
  <label label="string, required" storage_properties="uint2, required"/>
  <!-- One per component tag -->
  <component tag="uint8, required"/>
  <private>
    Hexadecimal content
  </private>
  <reserved_future_use>
    Hexadecimal content
  </reserved_future_use>
</application_recording_descriptor>
----
