==== EAS_inband_exception_channels_descriptor

Defined by ANSI/SCTE in <<SCTE-18>>.
Must be in a Cable Emergency Alert Table (table id 0xD8).

[source,xml]
----
<EAS_inband_exception_channels_descriptor>
  <!-- One entry per exception channel -->
  <exception RF_channel="uint8, required" program_number="uint16, required"/>
</EAS_inband_exception_channels_descriptor>
----
