==== RAR_over_IP_descriptor

Defined by DVB in <<ETSI-102-323>>.
Must be in a RNT (table id 0x79).

[source,xml]
----
<RAR_over_IP_descriptor
  first_valid_date="YYYY-MM-DD hh:mm:ss, required"
  last_valid_date="YYYY-MM-DD hh:mm:ss, required"
  weighting="uint6, required"
  complete_flag="bool, required"
  url="string, required"/>
----
