==== Program Map Table (PMT)

Defined by MPEG in <<ISO-13818-1>>.

[source,xml]
----
<PMT version="uint5, default=0"
     current="bool, default=true"
     service_id="uint16, required"
     PCR_PID="uint13, default=0x1FFF">

  <!-- Program-level descriptors -->
  <DESCRIPTOR_LIST>

  <!-- One per elementary stream -->
  <component stream_type="uint8, required" elementary_PID="uint13, required">
    <DESCRIPTOR_LIST>
  </component>

</PMT>
----
