==== Selection Information Table (SIT)

Defined by DVB in <<ETSI-300-468>>.

[source,xml]
----
<selection_information_table version="uint5, default=0" current="bool, default=true">

  <!-- Common descriptors loop, for transmission parameters -->
  <DESCRIPTOR_LIST>

  <!-- One per service -->
  <service service_id="uint16, required"
           running_status="undefined|not-running|starting|pausing|running|off-air,
                           required">
    <DESCRIPTOR_LIST>
  </service>

</selection_information_table>
----
