==== Application Information Table (AIT)

Defined by DVB in <<ETSI-102-809>> and <<ETSI-101-812>>.

[source,xml]
----
<AIT version="uint5, default=0"
     current="bool, default=true"
     test_application_flag="bool, default=true"
     application_type="uint15, required">

  <!-- Common descriptors loop -->
  <DESCRIPTOR_LIST>

  <!-- One per application -->
  <application control_code="uint8, required">
    <application_identifier
         organization_id="uint32, required"
         application_id="uint16, required"/>
    <DESCRIPTOR_LIST>
  </application>

</AIT>
----
