==== MPEGH_3D_audio_config_descriptor

Defined by MPEG in <<ISO-13818-1>>.

The _mpegh3daConfig_ structure is defined in <<ISO-23008-3>>.
Currently, it can only be represented as a binary blob in hexadecimal characters.
Some future version may be able to describe the internal structure of this data block.

[source,xml]
----
<MPEGH_3D_audio_config_descriptor>
  <mpegh3daConfig>
    Hexadecimal content
  </mpegh3daConfig>
</MPEGH_3D_audio_config_descriptor>
----
