==== EAS_metadata_descriptor

Defined by ANSI/SCTE in <<SCTE-164>>.
Must be in a Cable Emergency Alert Table (table id 0xD8).

[source,xml]
----
<EAS_metadata_descriptor fragment_number="uint8, default=1">
  <!-- The text inside this element is an XML fragment -->
</EAS_metadata_descriptor>
----
