==== cpcm_delivery_signalling_descriptor

Defined by DVB in <<ETSI-102-825-4>> and <<ETSI-102-825-9>>.

[source,xml]
----
<cpcm_delivery_signalling_descriptor cpcm_version="uint8, required">

  <cpcm_v1_delivery_signalling
      copy_control="uint3, required"
      do_not_cpcm_scramble="bool, required"
      viewable="bool, required"
      move_local="bool, required"
      move_and_copy_propagation_information="uint2, required"
      view_propagation_information="uint2, required"
      remote_access_record_flag="bool, required"
      export_beyond_trust="bool, required"
      disable_analogue_sd_export="bool, required"
      disable_analogue_sd_consumption="bool, required"
      disable_analogue_hd_export="bool, required"
      disable_analogue_hd_consumption="bool, required"
      image_constraint="bool, required"
      view_window_start="YYYY-MM-DD hh:mm:ss, optional"
      view_window_end="YYYY-MM-DD hh:mm:ss, optional"
      view_period_from_first_playback="uint16, optional"
      simultaneous_view_count="uint8, optional"
      remote_access_delay="uint16, optional"
      remote_access_date="YYYY-MM-DD hh:mm:ss, optional">

    <cps C_and_R_regime_mask="uint8, required">
      Hexadecimal Content
    </cps>

  </cpcm_v1_delivery_signalling>

</cpcm_delivery_signalling_descriptor>
----
