==== target_IPv6_slash_descriptor

Defined by DVB in <<ETSI-301-192>>.
Must be in an INT (table id 0x4C).

[source,xml]
----
<target_IPv6_slash_descriptor>
  <!-- One per IPv6 address: -->
  <address
      IPv6_addr="IPv6 address, required"
      IPv6_slash_mask="uint8, required"/>
</target_IPv6_slash_descriptor>
----
