==== parental_rating_descriptor

Defined by DVB in <<ETSI-300-468>>.

[source,xml]
----
<parental_rating_descriptor>
  <!-- One per country -->
  <country country_code="char3, required" rating="uint8, required"/>
</parental_rating_descriptor>
----
