==== Resolution provider Notification Table (RNT)

Defined by DVB in <<ETSI-102-323>>.

[source,xml]
----
<RNT version="uint5, default=0"
     current="bool, default=true"
     context_id="uint16, required"
     context_id_type="uint8, required">

  <DESCRIPTOR_LIST>

  <!-- One per resolution provider -->
  <resolution_provider name="string, required">

    <DESCRIPTOR_LIST>

    <!-- One per CRID authority -->
    <CRID_authority name="string, required" policy="uint2, required">
      <DESCRIPTOR_LIST>
    </CRID_authority>

  </resolution_provider>

</RNT>
----
