==== TS_information_descriptor

Defined by ARIB in <<ARIB-B10J>>.

[source,xml]
----
<TS_information_descriptor
    remote_control_key_id="uint8, required"
    ts_name="string, required">

  <!-- Up to 3 transmission types -->
  <transmission_type transmission_type_info="uint8, required">
    <service id="uint16, required"/>
  </transmission_type>

  <reserved_future_use>
    Hexadecimal content
  </reserved_future_use>

</TS_information_descriptor>
----
