==== Running Status Table (RST)

Defined by DVB in <<ETSI-300-468>>.

[source,xml]
----
<RST>
  <!-- One per event -->
  <event transport_stream_id="uint16, required"
         original_network_id="uint16, required"
         service_id="uint16, required"
         event_id="uint16, required"
         running_status="undefined|not-running|starting|pausing|running|off-air,
                         required"/>
</RST>
----
