==== short_smoothing_buffer_descriptor

Defined by DVB in <<ETSI-300-468>>.

[source,xml]
----
<short_smoothing_buffer_descriptor
    sb_size="uint2, required"
    sb_leak_rate="uint6, required">

  Hexadecimal content (optional DVB-reserved data)

</short_smoothing_buffer_descriptor>
----
