==== area_broadcasting_information_descriptor

Defined by ARIB in <<ARIB-B10J>>.

[source,xml]
----
<area_broadcasting_information_descriptor>

  <!-- One per station -->
  <station
      station_id="uint24, required"
      location_code="uint16, required"
      broadcast_signal_format="uint8, required">

    <additional_station_info>
      Hexadecimal content
    </additional_station_info>

  </station>

</area_broadcasting_information_descriptor>
----
