==== RAR_over_DVB_stream_descriptor

Defined by DVB in <<ETSI-102-323>>.
Must be in a RNT (table id 0x79).

[source,xml]
----
<RAR_over_DVB_stream_descriptor
  first_valid_date="YYYY-MM-DD hh:mm:ss, required"
  last_valid_date="YYYY-MM-DD hh:mm:ss, required"
  weighting="uint6, required"
  complete_flag="bool, required"
  transport_stream_id="uint16, required"
  original_network_id="uint16, required"
  service_id="uint16, required"
  component_tag="uint8, required"
  download_start_time="YYYY-MM-DD hh:mm:ss,
      optional group with download_period_duration and download_cycle_time"
  download_period_duration="uint8,
      optional group with download_start_time and download_cycle_time"
  download_cycle_time="uint8,
      optional group with download_start_time and download_period_duration"/>
----
