==== DII_location_descriptor

Defined by DVB in <<ETSI-101-812>>.
Must be in an AIT (table id 0x74).

[source,xml]
----
<DII_location_descriptor transport_protocol_label="uint8, required">
  <!-- One per module -->
  <module DII_identification="uint15, required" association_tag="uint16, required"/>
</DII_location_descriptor>
----
