==== cell_list_descriptor

Defined by DVB in <<ETSI-300-468>>.

[source,xml]
----
<cell_list_descriptor>

  <!-- One per cell -->
  <cell cell_id="uint16, required"
        cell_latitude="int16, required"
        cell_longitude="int16, required"
        cell_extent_of_latitude="uint12, required"
        cell_extent_of_longitude="uint12, required">

    <!-- One per subcell -->
    <subcell cell_id_extension="uint8, required"
             subcell_latitude="int16, required"
             subcell_longitude="int16, required"
             subcell_extent_of_latitude="uint12, required"
             subcell_extent_of_longitude="uint12, required"/>
  </cell>

</cell_list_descriptor>
----
