==== C2_bundle_delivery_system_descriptor

Defined by DVB in <<ETSI-300-468>>.

[source,xml]
----
<C2_bundle_delivery_system_descriptor>
  <!-- One per PLP -->
  <plp plp_id="uint8, required"
       data_slice_id="uint8, required"
       C2_system_tuning_frequency="FrequencyHz, required"
       C2_system_tuning_frequency_type="uint2, required"
       active_OFDM_symbol_duration="uint3, required"
       guard_interval="1/128|1/64|uint3, required"
       master_channel="bool, required"/>
</C2_bundle_delivery_system_descriptor>
----
