==== target_MAC_address_range_descriptor

Defined by DVB in <<ETSI-301-192>>.
Must be in an INT (table id 0x4C).

[source,xml]
----
<target_MAC_address_range_descriptor>
  <!-- One per MAC address range: -->
  <range MAC_addr_low="MAC address, required"
         MAC_addr_high="MAC address, required"/>
</target_MAC_address_range_descriptor>
----
