==== video_depth_range_descriptor

Defined by DVB in <<ETSI-300-468>>.

[source,xml]
----
<video_depth_range_descriptor>

  <!-- One per video range -->
  <range range_type="uint8, required"
         video_max_disparity_hint="int12, required when range_type == 0"
         video_min_disparity_hint="int12, required when range_type == 0">
    <range_selector>
      Hexadecimal content
    </range_selector>
  </range>

</video_depth_range_descriptor>
----
