==== Broadcaster Information Table (BIT)

Defined by ARIB in <<ARIB-B10>>.

[source,xml]
----
<BIT version="uint5, default=0"
     current="bool, default=true"
     original_network_id="uint16, required"
     broadcast_view_propriety="bool, required">

  <!-- Common descriptors loop -->
  <DESCRIPTOR_LIST>

  <!-- One per broadcaster -->
  <broadcaster broadcaster_id="uint8, required">
    <DESCRIPTOR_LIST>
  </broadcaster>

</BIT>
----
