==== splice_avail_descriptor

Defined by ANSI/SCTE in <<SCTE-35>>. Must be in a Splice Information Table (table id 0xFC).

[source,xml]
----
<splice_avail_descriptor
    identifier="uint32, default=0x43554549"
    provider_avail_id="uint32, required"/>
----
