==== data_broadcast_id_descriptor

Defined by DVB in <<ETSI-300-468>>.

[source,xml]
----
<data_broadcast_id_descriptor data_broadcast_id="uint16, required">
  <selector_bytes>Hexadecimal content</selector_bytes>
</data_broadcast_id_descriptor>
----
