==== CA_EMM_TS_descriptor

Defined by ARIB in <<ARIB-B25>>.

[source,xml]
----
<CA_EMM_TS_descriptor
    CA_system_id="uint16, required"
    transport_stream_id="uint16, required"
    original_network_id="uint16, required"
    power_supply_period="uint8, required"/>
----
