==== cue_identifier_descriptor

Defined by ANSI/SCTE in <<SCTE-35>>.

[source,xml]
----
<cue_identifier_descriptor
     cue_stream_type="insert_null_schedule|all|segmentation|tiered_splicing|
                      tiered_segmentation|uint8, required">
  <!-- Defined by SCTE 35 for use in PMT -->
</cue_identifier_descriptor>
----
