//----------------------------------------------------------------------------
//
// TSDuck - The MPEG Transport Stream Toolkit
// Copyright (c) 2005-2025, Thierry Lelegard
// BSD-2-Clause license, see LICENSE.txt file or https://tsduck.io/license
//
// Documentation paragraph for service parameters.
//
// tags: <none>
//
//----------------------------------------------------------------------------

[.optdoc]
If the parameter is an integer value (either decimal or hexadecimal), it is interpreted as a service id.
If its format is `_integer.integer_`, it is interpreted as major and minor ids on ATSC streams.
Otherwise, the parameter is interpreted as a service name, as specified in the SDT (DVB, ISDB) or VCT (ATSC).
Service names are not case sensitive and blanks are ignored.
If the input TS does not contain an SDT (DVB, ISDB) or VCT (ATSC), use a service id.
