==== service_prominence_descriptor

Defined by DVB in <<ETSI-300-468>>.

[source,xml]
----
<service_prominence_descriptor>

  <sogi
      SOGI_flag="bool, required"
      SOGI_priority="uint12, required"
      service_id="uint16, optional">

    <target_region
        country_code="string, optional"
        primary_region_code="uint8, optional"
        secondary_region_code="uint8, optional"
        tertiary_region_code="uint8, optional"/>

  </sogi>

  <private_data>
    Hexadecimal Content
  </private_data>

</service_prominence_descriptor>
----
