//----------------------------------------------------------------------------
//
// TSDuck - The MPEG Transport Stream Toolkit
// Copyright (c) 2005-2025, Thierry Lelegard
// BSD-2-Clause license, see LICENSE.txt file or https://tsduck.io/license
//
// Documentation for options in class ts::AbstractTablePlugin.
//
// tags: bat, cat, nit, pat, pmt, sdt
//
//----------------------------------------------------------------------------

//---- ugly tag tricks ----

:opt-table: table
:opt-bitrate: 3000
:opt-short-bitrate: true
:opt-short-increment: true
:!opt-optional:
// tag::pat[]
:opt-table: PAT
:!opt-short-bitrate:
// end::pat[]
// tag::cat[]
:opt-table: CAT
:opt-optional: true
// end::cat[]
// tag::pmt[]
:opt-table: PMT
:!opt-short-increment:
// end::pmt[]
// tag::sdt[]
:opt-table: SDT
// end::sdt[]
// tag::nit[]
:opt-table: NIT
// end::nit[]
// tag::bat[]
:opt-table: BAT
:opt-optional: true
// end::bat[]

//---- end of tag tricks ----

[.usage]
Generic options for table manipulation

[.opt]
ifdef::opt-short-bitrate[]
*-b* _value_ +
endif::[]
*--bitrate* _value_

[.optdoc]
Specifies the bitrate in bits / second of the PID containing the {opt-table} if a new one is created.

[.optdoc]
See xref:bitrates[xrefstyle=short] for more details on the representation of bitrates.

[.optdoc]
The default is {opt-bitrate} b/s.

[.opt]
*-c* +
*--create*

[.optdoc]
Create a new empty {opt-table} if none was received after one second.

[.optdoc]
This is equivalent to `--create-after 1000`.

[.opt]
*--create-after* _milliseconds_

[.optdoc]
Create a new empty {opt-table} if none was received after the specified number of milliseconds.
If an actual {opt-table} is received later, it will be used as the base for transformations instead of the empty one.

ifdef::opt-optional[]
[.optdoc]
This can be useful to force the creation of a {opt-table} in a TS which has none (the {opt-table} is an optional table).
endif::[]

[.opt]
ifdef::opt-short-increment[]
*-i* +
endif::[]
*--increment-version*

[.optdoc]
Increment the version number of the {opt-table}.

[.opt]
*--inter-packet* _value_

[.optdoc]
When a new {opt-table} is created and `--bitrate` is not present,
this option specifies the packet interval for the {opt-table} PID,
that is to say the number of TS packets in the transport between two packets of the PID.

[.optdoc]
Use instead of `--bitrate` if the global bitrate of the TS cannot be determined.

[.opt]
*--patch-xml* _filename_

[.optdoc]
Specify an XML patch file which is applied to each {opt-table} on the fly.
The XML patches are applied first.
The other options of this plugin are applied on the patched table.

[.optdoc]
If the specified name starts with `<?xml`, it is considered as inline XML content,
meaning that the string in the command line is directly the XML content and not a file name.

[.optdoc]
Several `--patch-xml` options can be specified.
Patch files are sequentially applied on each table.

[.optdoc]
See xref:xml-patch[xrefstyle=short] for more details on XML patch files.

[.opt]
*-v* _value_ +
*--new-version* _value_

[.optdoc]
Specify a new value for the version of the {opt-table}.
