==== target_IP_address_descriptor

Defined by DVB in <<ETSI-301-192>> and <<ETSI-102-006>>.
Must be in a UNT (table id 0x4B) or INT (table id 0x4C).

[source,xml]
----
<target_IP_address_descriptor IPv4_addr_mask="IPv4 address, required">
  <!-- One per IPv4 address: -->
  <address IPv4_addr="IPv4 address, required"/>
</target_IP_address_descriptor>
----
