==== ISP_access_mode_descriptor

Defined by DVB in <<ETSI-301-192>>.
Must be in an INT (table id 0x4C).

[source,xml]
----
<ISP_access_mode_descriptor access_mode="unused|dialup|uint8, required"/>
----
